               **************************************************
                      Myson MTD80X Based Fast Ethernet Card
                                 NDIS/5 Driver
                       Windows XP Installation Guide
               **************************************************

-----------------------
Installation Procedure 
-----------------------

 1. Plug the adapter into one of the Bus Master PCI slots of your PC.

 2. Power on your PC.

 3. Bring up Windows XP operating system.

 4. Windows XP will prompt for the "PCI Ethernet Controller" in "Found New 
    Hardware Wizard" dialog box.  Click the <NEXT> button.

 5. Select "Search for a suitable driver for my device" from "Found New 
    Hardware Wizard" dialog box, then click the <NEXT> button.

 6. Select "Specify a location" from "Optional search locations:" of 
    "Found New Hardware Wizard" dialog box, then click the <NEXT> button.

 7. Insert "Myson MTD80X Based Fast Ethernet Card" driver disk in the floppy 
    disk drive (e.g. A:)..

 8. Enter the driver path name as shown below, then click the <NEXT> button 
    from "Found New Hardware Wizard" dialog box.

      Example :

             A:\WINXP
      
 9. Select "Myson MTD80X Based Fast Ethernet Card",
    then click the <NEXT> button from the dialog box.

10. To complete the process, please follow the instructions on the screen.


 

