; DISPLAY P20-2S.INF Ver. 1.3.0.0
;Monitor INF file for Fujitsu Display P20-2S
;Copyright 2009 Fujitsu Technology Solutions

[Version]
signature="$CHICAGO$"
Class=Monitor
ClassGuid={4D36E96E-E325-11CE-BFC1-08002BE10318}
Provider=%FTS.Mfg%
CatalogFile=FTSP202S.cat
DriverVer=06/19/2009, 1.3.0.0

;-------------------------------------------------
[ControlFlags]
ExcludeFromSelect.nt=Monitor\FUS0554

[DestinationDirs]
DefaultDestDir=11

[SourceDisksNames]
1=%DISK%,,,

; Manufacturers
;-------------------------------------------------
[Manufacturer]
%FTS.Mfg%=FTS.Mfg,NTAMD64

; Manufacturer sections
;-------------------------------------------------
[FTS.Mfg]
%FUS-P20-2S%=FUS-P20-2S.Install, Monitor\FUS0554

[FTS.Mfg.NTAMD64]
%FUS-P20-2S%=FUS-P20-2S.Install, Monitor\FUS0554

; Install Sections
;-------------------------------------------------
[FUS-P20-2S.Install]
DelReg=DEL_CURRENT_REG
AddReg=FUS-P20-2S.AddReg, 1600, DPMS

; AddReg & DELReg sections
;-------------------------------------------------
[DEL_CURRENT_REG]
HKR,MODES
HKR,,MaxResolution
HKR,,DPMS
HKR,,ICMProfile

; Pre-defined AddReg sections

[1600]
HKR,,MaxResolution,,"1600,1200"

[DPMS]
HKR,,DPMS,,1

; AddReg sections
;-------------------------------------------------
[FUS-P20-2S.AddReg]
HKR,"MODES\1600,1200",Mode1,,"30-82,51-75,+,+"
HKR,,ICMProfile,0,"sRGB Color Space Profile.icm"

;-------------------------------------------------

[Strings]
DISK="Fujitsu Driver & Utility CD for DISPLAY P20-2S"
MonitorClassName="Monitor"
FTS.Mfg="Fujitsu Technology Solutions"
FUS-P20-2S="FUJITSU P20-2S"